(module SGC3 (layer F.Cu) (tedit 58B723CA)
  (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
  (tags "capacitor 0402")
  (attr smd)
  (fp_text reference REF** (at 0 -3.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SGC3 (at 0 3.429) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.2 2.2) (end -1.1 2.2) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.2 2.2) (end -1.6 1.8) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.6 1.8) (end -1.6 -2.2) (layer F.SilkS) (width 0.2032))
  (fp_line (start -1.6 -2.2) (end -1.1 -2.2) (layer F.SilkS) (width 0.2032))
  (fp_line (start 1.6 1.8) (end 1.6 -2.2) (layer F.SilkS) (width 0.2032))
  (fp_line (start 1.6 1.8) (end 1.2 2.2) (layer F.SilkS) (width 0.2032))
  (fp_line (start 1.2 2.2) (end 1.1 2.2) (layer F.SilkS) (width 0.2032))
  (fp_line (start 1.6 -2.2) (end 1.1 -2.2) (layer F.SilkS) (width 0.2032))
  (pad 1 smd rect (at 0 1.8375) (size 1.4 1.075) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0 -1.8375) (size 1.4 1.075) (layers F.Cu F.Paste F.Mask))
  (model ${KIPRJMOD}/ScopefunPackages3D/TZC3.wrl
    (at (xyz 0 0 0))
    (scale (xyz 0.3937 0.3937 0.3937))
    (rotate (xyz 0 0 0))
  )
)
