(export (version D)
  (design
    (source C:\Users\emone\OneDrive\kicad\AOZ2151QI_evaluation\AOZ2151QI_evaluation.sch)
    (date "3/16/2020 9:32:15 PM")
    (tool "Eeschema (5.1.5)-3")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source AOZ2151QI_evaluation.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value AOZ2151QI-01)
      (footprint KICAD_LIBRARY:QFN-20_3x3_Pitch0.5mm)
      (datasheet http://www.aosmd.com/res/data_sheets/AOZ2151QI-01.pdf)
      (libsource (lib AOZ2151QI-01) (part AOZ2151QI-01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F0170A3))
    (comp (ref C1)
      (value 1u)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F01DCE4))
    (comp (ref C2)
      (value 22u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F027C96))
    (comp (ref C4)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F028198))
    (comp (ref C5)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F035924))
    (comp (ref R2)
      (value 150K)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F05121A))
    (comp (ref C7)
      (value 22u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F05D86E))
    (comp (ref C8)
      (value 22u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F0E3121))
    (comp (ref C3)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F115557))
    (comp (ref L1)
      (value NR10050T4R9N)
      (footprint SamacSys_Parts2:NR10050T150M)
      (datasheet https://ds.yuden.co.jp/TYCOMPAS/ut/detail?u=M&pn=NR10050T4R9N)
      (fields
        (field (name Description) "TAIYO YUDEN - NR10050T4R9N - INDUCTOR, HIGH CURRENT WOUND, 4.9uH 30%, T&R 87K4744")
        (field (name Manufacturer_Name) "TAIYO YUDEN")
        (field (name Manufacturer_Part_Number) NR10050T4R9N)
        (field (name "Mouser Part Number") 963-NR10050T4R9N)
        (field (name "Mouser Price/Stock") https://www.mouser.com/Search/Refine.aspx?Keyword=963-NR10050T4R9N))
      (libsource (lib SamacSys_Parts) (part NR10050T4R9N) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E75EA7F))
    (comp (ref J1)
      (value Conn_01x05_Male)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x05_Male) (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E766D2B))
    (comp (ref C6)
      (value 22p)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F0661B2))
    (comp (ref R1)
      (value 110K)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F04CF1E))
    (comp (ref C9)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F0D4C2F)))
  (libparts
    (libpart (lib AOZ2151QI-01) (part AOZ2151QI-01)
      (fields
        (field (name Reference) U)
        (field (name Value) AOZ2151QI-01))
      (pins
        (pin (num 1) (name PGOOD) (type output))
        (pin (num 2) (name FB) (type input))
        (pin (num 3) (name AGND) (type input))
        (pin (num 4) (name IN) (type input))
        (pin (num 5) (name IN) (type input))
        (pin (num 6) (name IN) (type input))
        (pin (num 7) (name IN) (type input))
        (pin (num 8) (name IN) (type input))
        (pin (num 9) (name LX) (type output))
        (pin (num 10) (name PGND) (type input))
        (pin (num 11) (name PGND) (type input))
        (pin (num 12) (name PGND) (type input))
        (pin (num 13) (name LX) (type output))
        (pin (num 14) (name LX) (type output))
        (pin (num 15) (name EN) (type input))
        (pin (num 16) (name BST) (type input))
        (pin (num 17) (name VCC) (type output))
        (pin (num 18) (name SS) (type input))))
    (libpart (lib Connector) (part Conn_01x05_Male)
      (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x05_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib SamacSys_Parts) (part NR10050T4R9N)
      (fields
        (field (name Reference) L)
        (field (name Value) NR10050T4R9N)
        (field (name Footprint) NR10050T150M)
        (field (name Datasheet) https://ds.yuden.co.jp/TYCOMPAS/ut/detail?u=M&pn=NR10050T4R9N)
        (field (name Description) "TAIYO YUDEN - NR10050T4R9N - INDUCTOR, HIGH CURRENT WOUND, 4.9uH 30%, T&R 87K4744")
        (field (name Manufacturer_Name) "TAIYO YUDEN")
        (field (name Manufacturer_Part_Number) NR10050T4R9N)
        (field (name "Mouser Part Number") 963-NR10050T4R9N)
        (field (name "Mouser Price/Stock") https://www.mouser.com/Search/Refine.aspx?Keyword=963-NR10050T4R9N))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical AOZ2151QI-01)
      (uri C:\Users\emone\OneDrive\kicad\KICAD_LIBRARY/AOZ2151QI-01.lib))
    (library (logical Connector)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector.lib"))
    (library (logical Device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Device.lib"))
    (library (logical SamacSys_Parts)
      (uri C:\Users\emone\OneDrive\kicad\KICAD_LIBRARY/SamacSys_Parts.pretty/SamacSys_Parts.lib)))
  (nets
    (net (code 1) (name "Net-(C3-Pad1)")
      (node (ref C3) (pin 1))
      (node (ref U1) (pin 18)))
    (net (code 2) (name GND)
      (node (ref U1) (pin 10))
      (node (ref C4) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref U1) (pin 11))
      (node (ref J1) (pin 4))
      (node (ref C9) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U1) (pin 3))
      (node (ref U1) (pin 12))
      (node (ref C8) (pin 2))
      (node (ref C3) (pin 2)))
    (net (code 3) (name VINPG)
      (node (ref J1) (pin 2))
      (node (ref U1) (pin 15)))
    (net (code 4) (name "Net-(C1-Pad1)")
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 17)))
    (net (code 5) (name 5.0VCCIOPG)
      (node (ref J1) (pin 1))
      (node (ref U1) (pin 1)))
    (net (code 6) (name "Net-(C5-Pad1)")
      (node (ref U1) (pin 16))
      (node (ref C5) (pin 1)))
    (net (code 7) (name "Net-(C6-Pad2)")
      (node (ref R2) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref C6) (pin 2)))
    (net (code 8) (name VIN)
      (node (ref U1) (pin 7))
      (node (ref U1) (pin 4))
      (node (ref U1) (pin 5))
      (node (ref U1) (pin 6))
      (node (ref U1) (pin 8))
      (node (ref C2) (pin 1))
      (node (ref J1) (pin 3))
      (node (ref C4) (pin 1)))
    (net (code 9) (name 5.0VCCIO)
      (node (ref J1) (pin 5))
      (node (ref C9) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref L1) (pin 2)))
    (net (code 10) (name "Net-(C5-Pad2)")
      (node (ref C5) (pin 2))
      (node (ref L1) (pin 1))
      (node (ref U1) (pin 9))
      (node (ref U1) (pin 14))
      (node (ref U1) (pin 13)))))